Product

Last edited: 2025-10-02

# Packaging

## Master Case

Dfahlkfjhasldkjfhsdakjhf

**\_\_\_\_\_\_PASS \_\_\_\_\_\_FAIL**

Packaging

## Inner Case

Dfahlkfjhasldkjfhsdakjhf

**\_\_\_\_\_\_PASS \_\_\_\_\_\_FAIL**

Packaging

## Product Box

Dfahlkfjhasldkjfhsdakjhf

**\_\_\_\_\_\_PASS \_\_\_\_\_\_FAIL**

# Contents

## Prints

Dfahlkfjhasldkjfhsdakjhf

**\_\_\_\_\_\_PASS \_\_\_\_\_\_FAIL**

# Cosmetics

## Prints

Dfahlkfjhasldkjfhsdakjhf

**\_\_\_\_\_\_PASS \_\_\_\_\_\_FAIL**

# Function

## Prints

Dfahlkfjhasldkjfhsdakjhf

**\_\_\_\_\_\_PASS \_\_\_\_\_\_FAIL**

# Hardware

## Prints

Dfahlkfjhasldkjfhsdakjhf

**\_\_\_\_\_\_PASS \_\_\_\_\_\_FAIL**

# Smell

## Packaging

Any noticeable smell that would be considered foul or unpleasant would be cause for failure of this test. The following smells have occurred in the past and must be specifically checked for and never be present; Plastic Odor, Burnt Plastic Odor, or Chemical or Solvent Odor. The following packing materials should be checked.

• Shipping Carton

• Poly Bags

• Plastic Protective Coverings

• Instruction Manual

**\_\_\_\_\_\_PASS \_\_\_\_\_\_FAIL**

Smell

## Hardware

Any noticeable smell that would be considered foul or unpleasant would be cause for failure of this test. The following smells have occurred in the past and must be specifically checked for and never be present; Plastic Odor, Burnt Plastic Odor, or Chemical or Solvent Odor. The following hardware should be checked.

**\_\_\_\_\_\_PASS \_\_\_\_\_\_FAIL**

# Version History

## 2025-10-01

Creation, Combining Inspection Documents: Express 2.0L, Express 1.4L, Cold Brew 360 2.0L, and Cold Brew 1.4L. | Removed repeated sections |